Web Integration - Active Units - IP Load Balancing

Home >> Web Integration >> Active Units - IP Load Balancing

Our Principals

| Cisco local Director / Distributed Director
| Ms - WLBS

Function

| Load - Balancing TCP or UDP Servers.
| High performance to handle high-traffic web sites.
| High availability for mission - critical applications.
| Load distribution across geographically / topologically dispersed TCP / IP Servers.
| High availability for dispersed mission - critical applications.
| Data center redundancy & failover.
| TN3270 sessions in an IBM environment.

Features & Benefits

| Hot stand by & state ful failover enables configuration of highly redundant system.
| Server & application probing for fail-over on a per-port basis.
| Scalable to meet the needs of largest web sites.
| Configurable to a total of 64,000 virtual & real servers, offers flexibility in domain names & network configuration.
| Up to 240 Mbps throughput & over 20,000 connections/sec.
| SSL, Cookie stiky, Redirect sticky ensure completion of complex transactions in proxy server.
| Transparent distribution of all IP Services (TCP & UDP) including HTTP, FTP, Telnet provides global scalability for all IP based networks.
| Leverages Routing Table Information (BGP & IGP) in the Network Infrastructure to make "Network Intelligent".
| Calculates client - to - server round-trip times in real time, redirects client is to server with lowest client - to - server link latency, maximizing end - to - end server access performance.
| Redirects clients only to responsive servers.
| Allows servers to be added & removed transparently, simplifying maintenance of distributed servers.
| Supports multiple domains, cost - effective IP Service scalability solution.

[ Web Integration | Software Development | System Integration | Support Services | Service Centre ]
[ About Us | Happenings | Partnerships | Jobs | Customers Speak | Site Map | Contact Us | Feedback | Home ]

© Ashtech Infotech Ltd. 2000. All rights reserved.
Best experienced with 800 x 600 screen resolution