Web Integration - Active Units - Switches

Home >> Web Integration >> Active Units - Switches

Our Principals

| Cisco Systems
| Nortel Networks / BayNetworks
| Extrance
| Cabletron
| D-Link
| 3Com

Function

| Bandwidth congestion on the network.
| High Traffice due to more no of users / servers, different projects etc.
| Application & protocols requiring high speed / bandwidth per user.
| Collisions are decreased because unicast frames are forwarded only out of the correct port.
| Concurrent frame forwarding is allowed.

Features & Benefits

| Reduces network traffic / conpestron by creating separate collision domains.
| Provides switched 10/100 Mbps to end users / desktops and 100 / 1000 Mbps for server farm.
| Better management of the network.
| Combines user Traffic to different LAN segments by segmentation.
| Switches are typically hardware optimized for speedy switching.

[ Web Integration | Software Development | System Integration | Support Services | Service Centre ]
[ About Us | Happenings | Partnerships | Jobs | Customers Speak | Site Map | Contact Us | Feedback | Home ]

© Ashtech Infotech Ltd. 2000. All rights reserved.
Best experienced with 800 x 600 screen resolution