Web Integration - Active Units - Routers

Home >> Web Integration >> Active Units - Routers

Our Principals

| Cisco Systmes
| Nortel Network / Baynetworks

Function

| To reduce broadcast, Multicast traffic to a particular LAN segments.
| Callisions are decreased because trances between devices on the same segment are not forwarded by routers.
| Routers provide seller landwidth per segment & mangeability as they have detail knowledge of the packet flow.

Features & Benefits

| Routers Provide more functioality e.g. packet fragmentation & reassenbly plus packet life the control.
| Distance limitatations are overcome because each segment can be built with the maximum distance for that type of Ethernet.
| Routers Perform switching of packets using layer 3 heders & logice.

To reduce broadcast, multicast traffic to a particular LAN Seg
servers from Sun Microsystems, Compaq and Hewlett Packard. Routers and switches from Cisco and Intel. Integrate on the Windows NT and Solaris and Linux platform. IP Load balancing products and Caching servers also form a part of our offering.

Microsystems
servers from Sun Microsystems, Compaq and Hewlett Packard. Routers and switches from Cisco and Intel. Integrate on the Windows NT and Solaris and Linux platform. IP Load balancing products and Caching servers also form a part of our offering.

[ Web Integration | Software Development | System Integration | Support Services | Service Centre ]
[ About Us | Happenings | Partnerships | Jobs | Customers Speak | Site Map | Contact Us | Feedback | Home ]

© Ashtech Infotech Ltd. 2000. All rights reserved.
Best experienced with 800 x 600 screen resolution